**SUPPLEMENTAL SPECIFICATION NO. 1**

**This Supplemental Specification amends the provisions of the Standard Specifications for Airport Construction, 2021 Edition, and shall be considered to be a part of those Standard Specifications, superseding any conflicting provisions in the Standard Specifications applicable to work under the Contract.**

**Modify Section 402.2.1 General (1): to remove the last sentence of “Do not regress air voids”**

The modified specification should read as follows:

402.2.1 General (1) Furnish a homogeneous mixture of coarse aggregate, fine aggregate, mineral filler if required, recycled material if used, warm mix asphalt additive or process if used, and asphaltic material.